
                             README.TXT File
    README file for EUTRON PocketReader Driver, Version 3.7.2.1
                Copyright (c) 2000 - 2001 OMNIKEY AG

This document describes the release notes of the EUTRON PocketReader Driver
(NOTE: to read this document with notepad enable the "word wrap" function)
===========================================================================


I. General
**********


PLEASE NOTE: NEVER INSTALL THE MICROSOFT SMART CARD BASE COMPONENTS 
MANUALLY!!(scbase.exe and smclib.exe)


Supported Operating Systems:
----------------------------

This driver supports the operating systems
Windows 98
Windows Millennium Edition (ME)
Windows 2000
Windows XP


II. Installation:
*****************

The installation will be done by PnP.
The 'New Hardware Found' dialog box will appear and you will be asked for
the driver location, where you have to select the source directory of the
driver files.

SPECIAL NOTE FOR Windows 2000 and Windows Millennium Edition (ME) USERS:
Please note that, if you have extracted the driver files to a folder on your
hard drive or network drive, you will have to specify the location of that
folder instead of the location "a:\" (the search on floppy wil be performed
automatically).
When you will be asked to search for a driver for the device, do not select
the recommended choice. Select the '...I can choose a specific driver' and
in the next window specify the location of the folder where you saved the
driver files.

At the same time, the CardMan Diagnostic Tool will be installed.
This tool is listed in the Control Panel and displays version and status
information.

You can remove the CardMan Diagnostic Tool by deleting the following files:
- For Windows 98 and Windows Millennium Edition (ME) cmdiag.cpl, cmdiag.ini,
cmabout.dll, cmabout.ini and eutron.bmp in the SYSTEM directory.
- For Windows 2000 cmdiag.cpl and cmdiag.ini in the SYSTEM32 directory.


MS Smart Card Base Components
-----------------------------

The PocketReader needs the Microsoft Smartcard Base Components for proper 
operation.

The Microsoft Smartcard Base Components are automatically installed by the
driver files Windows 98, Windows Millennium Edition (ME).

The Microsoft Smartcard Base Components are already integrated in Windows
2000 and XP.
If you have accidentally installed the Base Components under Windows 2000,
you can recover the smartcard subsystem with the following commands on an 
administrator's console window:
- Regsvr32 %windir%\system32\scardssp.dll
- Scardsvr reinstall
Note: You must no use this commands for XP ! They will not work

III. Updating:
**************

Windows 98 and Windows Millennium Edition (ME):
Because the Resource Manager does not support PnP, two message windows (two 
times:...Access is denied.) will appear during the update process.
Just press OK, restart, and everything is all right.

Windows 2000, Windows Millennium Edition (ME) and XP:
When asked how you want to update the driver, do not select the recommended 
choice. Select the '...I can choose a specific driver' and in the next
window select the newer driver.


IV. What is new in this release?
********************************
- FI/DI of 0x03 supported (rel. 3.7.2.1)
- improved buffer handling for low resources (rel. 3.7.1.1)


Release date: 28/11/2001

Revision date: 05/12/2001

-------------------------------- END OF FILE ------------------------------