
                             README.TXT File
    README file for EUTRON PocketReader Driver, Version 3.7.1.1
                Copyright (c) 2000 - 2001 OMNIKEY AG

This document describes the release notes of the EUTRON PocketReader Driver
=================================================================================


I. General
**********


PLEASE NOTE: NEVER INSTALL THE MICROSOFT SMART CARD BASE COMPONENTS 
MANUALLY!!(scbase.exe and smclib.exe)


Supported Operating Systems:
----------------------------

This driver supports the operating systems Windows 98,
Windows Millennium Edition (ME) and Windows 2000.


II. Installation
*****************

The installation will be done by PnP.
The 'New Hardware Found' dialog box will appear and you will be asked for the
driver location, where you have to select the source directory of the driver 
files.

SPECIAL NOTE FOR Windows 2000 and Windows Millennium Edition (ME) USERS:
Please note that, if you have extracted the driver files to a folder on your
hard drive or network drive, you will have to specify the location of that folder
instead of the location "a:\" (the search on floppy wil be performed automatically).
When you will be asked to search for a driver for the device, do not select the
recommended choice. Select the '...I can choose a specific driver' and in the next
window specify the location of the folder where you saved the driver files.

At the same time, the CardMan Diagnostic Tool will be installed. This tool is 
listed in the Control Panel and displays version and status information.

You can remove the CardMan Diagnostic Tool by deleting the following files: For 
Windows 98 and Windows Millennium Edition: : cmdiag.cpl, cmdiag.ini, cmabout.dll, 
cmabout.ini and eutron.bmp in the SYSTEM directory.
For Windows 2000: cmdiag.cpl and cmdiag.ini in the SYSTEM32 directory.


MS Smart Card Base Components:
------------------------------

The PocketReader needs the Microsoft Smartcard Base Components for proper 
operation.

The Microsoft Smartcard Base Components are automatically installed by the driver 
files for Windows 95, Windows 98, Windows Millennium Edition and Windows NT 4.0.

The Microsoft Smartcard Base Components are already integrated in Windows 2000. 
If you have accidentally installed the Base Components under Windows 2000, you 
can recover the smartcard subsystem with the following commands on an 
administrator's console window:
Regsvr32 %windir%\system32\scardssp.dll
Scardsvr reinstall


III. Updating:
**************

Windows 98 and Windows Millennium Edition (ME) :
Because the Resource Manager does not support PnP, two message windows (two 
times:...Access is denied.) will appear during the update process.
Just press OK, restart, and everything is all right.

Windows 2000 and Windows Millennium Edition (ME) :
When asked how you want to update the driver, do not select the recommended 
choice. Select the '...I can choose a specific driver' and in the next window 
select the newer driver.


IV. What is new in this release?
********************************

- improved buffer handling for low resources



Release date: 09/14/2001

Revision date: 05/10/2001

-------------------------------- END OF FILE -------------------------------
